                      =================================
                                Release Notice
                                ALi Corporation
                      =================================

-------------------------------------------------------------------------
Subject: M5632 (USB2.0 Host Link) Software Package
Version: 1.20 M
Date   : April,22, 2003

Contents:
 	Description
 	Change History
 	Setup Configuration

-------------------------------------------------------------------------
Description:

 Release M5632 Software Package Version 1.20 M

 Version features
  1:Improved on notebooks based on TI cardbus adapter
  2:Updated the firmware file.

 See Change History for detail.
-------------------------------------------------------------------------
Change History:
Version: 1.20 M
Date   : April,22, 2003
  1:Improved on notebooks based on TI cardbus adapter
  2:Updated the firmware file.

Version: 1.20 L
Date   : April,17, 2003
  1:Revise the issue of suspend of SuperLink.
  2:Enhance the function of detecting device in AP of SuperLink.

Version: 1.20 K
Date   : April,11, 2003
  1:Update the new M5633.bin.The new firmware supported two ways to control the LED. The customer can select to turn the LED     on or off from the EEPROM context.

Version: 1.20 J
Date   : April,4, 2003
  1:Update the new M5633.bin (ver 1.07) to turn on the LED too at the virtual network driver.

Version: 1.20 I
Date   : March,27, 2003
  1:SuperLink supports different vender ID and product ID by editing some files.(VirtualNetwork already supports it.)
  2:VirtualNetwork revised an issue that "Enhanced mode 32 Bit and 16 Bit NDIS Driver" option does not checked automatically 	    only under Windows Me.
  3:Installer revised a issue when installed from CD-ROM under windows 98SE/Me.

Version: 1.20 H
Date   : March,26, 2003
 1:SuperLink driver is modified for suspend issue.
 2:VirtualNetwork set the default frame size mode to "standard mode" under windows 9x.
 3:Installer cancelled binding NETBEUI protocol with VirtualNetwork under windows 2000
 4:ReleaseNotice addded "How to configure a different VIDPID of installer?"
 5:Readme.txt added section "Configure VirtualNetwork adapter".

Version: 1.20 G
Date   : March,19, 2003
 1:Firmware upgrade to 1.06 verison to turn LED always on

Version: 1.20 F
Date   : March,12, 2003
 1:Setup revised a bug under some windows me platform which will let user specify the path of firmware file
 2:SuperLink revised a bug when copy files between Unicode and not Unicode Version.

Version: 1.20 E
Date   : March,11, 2003
 1: SuperLink revised a bug when cut and overwrite read-only file.

Version: 1.20 D
Date   : March,10, 2003
 1: SuperLink revised a bug of paste.

Version: 1.20 C
Date   : March,09, 2003
 1: SuperLink revised a bug of NoAll.
 2: SuperLink revised copyright.

Version: 1.20 B
Date   : March,07, 2003

 1: SuperLink and VirtualNetwork driver solve the connection issue of notebooks installed TI and Ricoh cardbus.
 2: SuperLink remove a issue of time out when copying files.
 3: SuperLink remove a bug when cut and paste.
 4: SuperLink and Installer Support Japanese language.

Version: 1.20 A1
Date   : March,06, 2003
 1:Superlink removed the bug of Cancel.
 2:Installer revised something about reboot.
 3:When install microsoft bus driver based on TI cardbus, sending vendor command will cause system to crash. 
	SuperLink and VirtualNetwork driver of this version solves this problem.

Version: 1.20 A
Date   : March,05, 2003
 1:VirtualNetwork Revised boot bug under Windows 98SE/Me (TP0213)
 2:VirtualNetwork Added Bridge function under Windows 2000
 3:VirtualNetwork Added a Bridge switch/uninstall tool BridgeSwitch.exe
 4:Installer supports muti-language(English,Simplified Chinese,Traditional Chinese).
 5:Installer added the function of to bind the protocol of "File and Printer Sharing" automatically.
 6:Superlink supports muti-language(English,Simplified Chinese,Traditional Chinese).
 7.Superlink removed some connect timeout problem
 8.Superlink added sort function in ListView
 9.Superlink removed some display and mouse move bug
 10.Superlink uses move function when cut and paste files in same disk.
 11.Superlink removed delete dialog when cut and paste file.
 12.Superlink Removed a bug when copy folder.
 13.Superlink Remove one bug about connection.
 14.When install microsoft bus driver based on TI cardbus, sending vendor command will cause system to crash. 
	SuperLink and VirtualNetwork driver of this version solves this problem.

Version: 1.10 A
Date   : Feb,15, 2003
 1:Enhanced SuperLink.exe to improve performance
 2:Added the function of binding NETBEUI and TCPIP protocol when install VirtualNetwork.
 3:Revised the bug of clicking setup.exe fast more than once (TP0214)
 4:Revised the bug of setup under windows 98 setup will show a error message(TP0219)

Version 1.08 C:
Date   : Jan 23, 2003
 1:Enhanced SpuerLink to suspend from and resume to S3.
 2:Add the property page of VirtualNetwork,Let user to select the frame size mode of VirtualNetwork.If FTP speed is 
   slow,user can change the frame size mode from "turbo mode" to "standard mode".
 3:Revised the installer to support only one product.
	If delete the VirtualNetwork sub-folder,installer will skip the 1st page of selection,goto the install page 
	of SuperLink directly.
	If delete the SuperLink sub-folder,installer will skip the 1st page of selection,goto 	the install page of 
	VirtualNetwork directly.
 4:Revise the bug of installer under windows 98/Me that after installed the VirtualNetwork,there will be a unusefull
  "USB Virtual Network Adaper" added to the property page of network neighbor's adapter list.This version's installer
   deleted this idle device from the property page.
 5:Replace Vendor.BMP by the new Vendor.BMP.

Version 1.08 B:
Date   : Jan 20, 2003
 1:Revised SpuerLink to suspend from and resume to S3.
 2:Revised the dispaly bug of installer under big font

Version 1.08 A:
Date   : Jan 16, 2003
 1:Revised VirtualNetwork to suspend from and resume to S3.

Version 1.08:
Date   : Jan 16, 2003
 1:SpuerLink.exe supports Unicode version.
 2:Revised install to install two versions superLink.exe (UNICODE and ANSI)

Version 1.07:
Date   : Jan 13, 2003
 1:Update 5633.bin of version 1.04
 2:Revised a bug about installer when user specifies a error path to install.
 3:Backward compatibility with the installer after 1.02 version.
 4:Revised the Ulink.inf

Version 1.06:
Date   : Jan 7, 2002
 1:Added the notify FW  mechanism when suspend and reset interrupt pipe mechanism when resume in VirtualNetwork.
 2:Revised Ulink driver also in above aspect.
 3:Resolve error: "Can't  read" shows up when the selected file has been  opened by other application or is running of
   superlink.exe.
 4:Resolve error: In copying file from  remote to remote, if user cancels the operation, the system will halt of
   superlink.exe.
 5:Ameliorated Suspend / resume issue of superlink.exe and ulink.sys.
 6:Tuned up FTP transfer rate for VirtualNetwork.

Version 1.05:
Date   : Dec 31, 2002
 1. Ameliorate timeout problem
 2. vendor.bmp's width*height ration is set as 10:7
 3. some other improvement of installer

Version 1.04:
Date   : Dec 31, 2002
 1. Revised the bug of installer when files are set read-only.

Version 1.03:
Date   : Dec 26, 2002
 1. Revised one bug of installer when when user delete the "SuperLink" directory to run setup.exe, and run setup 
    again at start->program->USB VirtualNetwork>setup.exe.

Version 1.02:
Date   : Dec 26, 2002
 1:Changed readme.txt
 2:Changed install exe file into single setup.exe.
 3:Revised the superlink shortcut folder name from "SuperLink"to "USB SuperLink"

Version 1.01:
Date   : Dec 24, 2002
 1:ticker revised some bugs of superlink.exe
 2:add the shortcut and folder of ulan
 3:place all the other files of install to the "Share" folder,except 2 install executable files.
 4:avoid the digital signature dialog during install executable file running process under windows 2K.
-------------------------------------------------------------------------
Setup Configuration:

The Setup utility is configurable to provide manufacturers flexibility for satisfying
different marketing requirements. Here are configurable items

1.How to configure Setup utility as single solution or combo solution?

  M5632 USB Host Link supports dual software solutions, "USB Super Link" and "USB Virtual Network".
  Each software solution can be easily disabled by removing the related sub-directory,
  that is, manufacturers can flexibly make their own Software Package as desired,
  either a combo solution, or a single solution.
  
  For example, 
  If manufacturers want to ship the product with "USB Super Link" solution only, just need to
  delete the sub-directory "VirtualNetwork", vice versa, if manufacturers want to ship 
  product with "USB Virtual Network" solution only , just need to remove sub-directory 
  "USB Super Link". Or, keep both sub-directories for a combo solution release.

    
2.How to configure multilingual support ?
  M5632 Software Package supports multiple languages. The following notes tell manufacturers how to configure 
  multilingual support.

  Open "info.txt" file under sub-directory "share"
  
  Search the following statements
  
  	SupportedLanguageID=0409,0404,0804,0411
	DefaultLanguageID=0409

  These statements mean this release supports four languages, 0409,0404,0804,0411.
  	
  ( 0804: Traditional Chinese )
  ( 0404: Simplified Chinese )
  ( 0409: English )
  ( 0411: Japanese )
  
  The language support is configurable.	
  For example, if manufacturer only want to support English version, the statements will be modified as  
  
  	SupportedLanguageID=0409
	DefaultLanguageID=0409
3.How to configure a different VIDPID of installer?  
  If you need change the VIDPID to a new one,please edit the following 3 files:
  1:"root\share\info.txt"
	there are 2 lines about VIDPID.They are
		1: VIDPID=VID_0402&PID_5632
		2: VIDPID2=VID_0402&PID_5632
	Please replace VID_0402&PID_5632 with the new VIDPID.
  2:"root\VirtualNetwork\ULan.inf"
	There 2 lines about VIDPID.They are
	1: "%INTERMEDIATEDEVICE.DESCRIPTION% = Corp.Install, USB\VID_0402&PID_5632"
	2: "HKR,  Ndi,     DeviceID ,    , "USB\VID_0402&PID_5632" 
	Please replace VID_0402&PID_5632 with the new VIDPID.
  3:"root\SuperLink\ulink.inf"
	please replace "VID_0402&PID_5632" of the line 
	"%Usblink.a%=Usblink.Install,USB\VID_0402&PID_5632" with the new VIDPID

 ALL the VIDPID information of this 3 files must be consistent!
-------------------------------------------------------------------------
